{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["公开招标"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"公开招标","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"merged":[[0,0,0,5]]}
["北京按摩医院2026年康复类设备基本要求"]
["序号","科室","设备名称","数量","单位","基本要求"]
[1,"特需门诊","中频干扰电治疗仪",2,"台","适用镇痛，改善局部血液循环、促进炎症消散、软化瘢痕，松解黏连。至少分两组可独立调节输出，每组至少2通道，每通道为4个电极，有导子加热功能。"]
[2,"特需门诊","短波治疗仪",1,"台","适用于对人体进行止痛、消炎。分为两种治疗模式：持续和脉冲，脉冲输出调节为无极调节，脉冲重复频率可以在15—200Hz之间选择，分为不少于9个等级；快速自动调谐，保证功率输出恒定；在治疗过程中，由持续输出转为脉冲输出时设备自动停止输出；由脉冲输出转为连续输出，设备输出自动调节到最小安全值；全屏蔽设计，设备电源线为具有电磁屏蔽网的不可拆卸软电缆，具有良好的电磁兼容性，屏蔽有害电磁辐射。"]
[3,"特需门诊","人体成份分析仪",1,"台","采用多频率生物阻抗分析技术，将人体五个节段分别独立进行阻抗测量，从而计算和得出人体水分、蛋白质、脂肪等各个组成成分。"]
[4,"特需门诊","电动多功能理疗床",3,"台","床面分为头板、背板和腿板三部分，且三部分角度能分别独立调节，床面升降调节。"]
[5,"儿科","言语语言评估与康复系统",1,"台","适用于言语语言障碍、发育迟缓、听力障碍、孤独症谱系障碍等患者的言语语言功能的评估与康复治疗，涵盖几乎所有的言语语言障碍，可进行言语语言能力评估和康复训练， 基于游戏化、智能化的形式进行康复训练。"]
[6,"儿科","少年儿童生长发育干预改善运动处方系统",1,"台","提供了不同年龄儿童增高、减脂、体质改善、感统训练、体态改善等运动处方。"]
[7,"儿科","儿童书写障碍评估及干预体系",1,"台","通过智能化书写设备采集学龄儿童书写数据，然后将数据上传到云平台进行智能化分析，系统自动出具儿童书写能力综合报告，进行书写障碍康复技能培训。"]
[8,"儿科","医用诊疗床（电动升降PT床）",1,"张","床面分为头板、背板和腿板三部分，且三部分角度能分别独立调节，床面升降调节。"]
[9,"儿科","三维电子脊柱测量仪",1,"台","适用于自动化筛查与测量脊柱畸形、姿势异常及活动度范围。"]
[10,"儿科","经颅重复磁刺激仪",1,"台","刺激人体中枢神经和外周神经，用于人体中枢神经和外周神经功能的检测、评定、改善，对脑神经及神经损伤性疾病的辅助治疗。可用于儿童。"]
[11,"儿科","气动式关节康复训练仪",1,"台","适用于对上肢（手指、手腕）、下肢（脚踝）关节的康复性训练。多种训练模式可选择。"]
[12,"儿科","脑电仿生电刺激仪（儿童）",1,"台","磁疗部分与电疗部分既可同时使用，也可单独使用，多种模式可调"]
[13,"儿科","经络导平治疗仪",1,"台","可进行多穴位整体平衡治疗，具有短路保护功能；具有电极片脱落报警功能"]
[14,"儿科","半导体激光治疗仪",2,"台","双路独立控制"]
[15,"儿科","激光治疗仪",2,"台","整机有四组输出通道，每组都带负压自动吸附定位，激光结合拔罐功能，可同时提供两种物理康复治疗模式，每组独立工作，可依需求更换激光头"]
[16,"儿科","吸附式点刺激低频治疗仪",1,"台","吸附式电极、普通电极两种可供选择，具有短路、开路保护功能；具有电极片脱落报警功能"]
[17,"儿科","神经肌肉电刺激仪",1,"台","8路电极独立输出，可同时满足多人/多部位治疗需求"]
[18,"儿科","超声波治疗仪",1,"台","多种超声输出模式，双通道可同时输出"]
[19,"儿科","生物刺激反馈仪",1,"台","用于对患者的身体表面肌电信号进行采集、分析和生物反馈训练，辅助恢复患者肌肉功能障碍。独立4通道"]
[20,"康复科","手功能康复评估与训练系统",1,"套","适用于上肢和手指关节功能障碍患者的康复训练和辅助治疗，兴奋上肢肌肉组织，促进局部血液循环。\n多种训练模式，更具不同的患者选择不同的训练模式"]
[21,"康复科","低频交变磁场治疗机",1,"台","双通道磁场输出"]
[22,"康复科","床旁下肢主被动运动康复机",1,"台","用于卧床患者下肢的运动康复训练；多种训练模式可选择"]
[23,"康复科","床旁上肢主被动运动康复机",1,"台","用于患者上肢的运动康复训练；多种训练模式可选择"]
[24,"康复科","吸附式点刺激低频治疗仪",1,"台","吸附式电极、普通电极两种可供选择，具有短路、开路保护功能；具有电极片脱落报警功能"]
[25,"康复科","认知障碍评估训练与脑电刺激治疗系统\n（1拖4）",1,"套","轻度认知障碍、语言障碍等的辅助治疗，产品含有认知障碍评估训练软件，不同训练模块和训练场景"]
[26,"康复科","生物反馈电刺激工作站\n(1拖8)",1,"套","由主机针对每个患者设置个性化治疗方案，同一主机可以针对每个患者分别设置多台从机实现电刺激治疗，从机数量可选配8个"]
[27,"康复科","康复踏车",2,"台","设备提供动力、用户交互界面进行上肢及下肢功能康复训练，具有患者从完全被动训练阶段到主动和被动训练相交叉的助力训练阶段到完全的主动训练阶段到初期主动力量训练阶段的患者康复过程。具有痉挛保护功能。"]
[28,"康复科","无线表面肌电反馈仪",1,"台","常规表面肌电图的实时监测，肌电生物反馈治疗，以及肌肉的肌力评估和疲劳度评估。要求传感器可通过无线网络 (WiFi)进行数据传输，满足≥8通道 8K 高精度采 样率的同步稳定传输需求"]
[29,"康复科","呼吸神经肌肉刺激仪",1,"台","能同时对呼吸肌肉多部位进行电刺激训练，使呼吸肌肉系统进行规律性收缩，起到改善肺通气功能。"]
[30,"康复科","肺功能测试仪",1,"台","支持进行呼气肺功能检测指标，适用人群：成人"]
[31,"康复科","电动多功能理疗床",1,"张","床面分为头板、背板和腿板三部分，且三部分角度能分别独立调节，床面升降调节。"]